{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["市一梯控设备清单"],"not_rendered":{"images":4},"read":"whole","date_system":"1900"}

{"sheet":"市一梯控设备清单","index":0,"n_rows":13,"n_cols":9,"rows_kept":13,"merged":[[0,0,1,8]]}
["东湾绿城22号楼梯控报价单"]
[]
["序号","设备名称","品牌","型号","技术规格","单位","数量","备注","图片"]
[1,"读卡器","海康威视","DS-K1102M","认证方式：刷卡\n读卡频率：13.56MHz\n可识别卡：IC卡(支持扇区加密)、CPU卡序列号(不含加密功能)\n按键方式：无\n通讯方式：RS485+Wiegand\n工作电压：DC 12V\n功耗：≤2W\n安装方式：明式安装\n工作环境：室内\n设备尺寸：85.6mm(高)x86.5mm(宽)x29.6mm(厚)\n\n","台",6,"每台电梯配置1台，安装于电梯内",""]
[2,"梯控主机","海康威视","DS-K2210","支持web界面操作，最多控制128层电梯；\r\n支持接入2个Wiegand读卡器或RS485读卡器；\r\n支持2万张卡片管理，5万条事件存储；\r\n具有消防输入接口；\r\n带机箱和供电电源；\r\n工作电压：DC12V，50W（自带电源，AC220V输入）；\r\n尺寸：235*284*90mm。","台",6,"每台电梯配置1台，安装于电梯机房内",""]
[4,"梯控联动模块（32层）","海康威视","DS-K2M0032A","具有32个继电器输出；\r\n带机箱和供电电源；\r\n工作电压：DC12V，50W（自带电源，AC220V供电）\r\n尺寸：235*284*90mm","台",6,"每台电梯配置1台，安装于电梯顶",""]
[5,"海康威视管理平台软件","海康威视","梯控管理","梯控应用通过接入梯控设备，实现人员身份识别、楼层管控等智能应用；主要提供权限配置管理和事件管理应用。\n一、提供梯控权限管理应用\n1、支持按组织、人员维度配置梯控权限；\n2、支持梯控权限的增量下发和初始化下发；\n3、支持按周计划设置楼层常开常闭工作状态；\n4、支持按楼层、人员、组织、区域等多维度，综合查询权限配置、下发状态等信息；\n二、提供事件管理应用\n1、支持配置平台接收到事件类型；\n2、支持配置事件保存时长；\n3、支持查询人员出入事件和设备事件。","套",1,"1、支持管理梯控设备数量500个；\n2、支持最大梯控刷卡数据最大存储数量2000万条。",""]
[6,"RS-485 通讯线","国标","RVVP 2*1","用于联动模块和梯控主机通讯","米",600]
[7,"联动线","国标","RVVP 6*1 ","用于联动模块和梯控主机通讯","米",600]
[8,"开关量信号控制线","国标","RVV2*0.5","用于电梯按钮和联动模块通讯","米",800]
[9,"安装配件","国标",null,null,"项",1]
[10,"安装调试",{"$nulls":3},"项",1]
["合计报价(元)："]