{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["样衣参数","样衣模特数据参考"],"not_rendered":{"images":2,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"样衣参数","index":0,"n_rows":14,"n_cols":14,"rows_kept":14,"merged":[[0,2,0,13],[2,1,6,1],[2,3,3,3],[2,4,3,4],[2,7,11,7],[2,13,11,13],[5,3,6,3],[5,4,6,4],[7,1,11,1],[7,3,8,3],[7,4,8,4],[10,3,11,3],[10,4,11,4],[12,0,12,7],[13,0,13,13]],"flags":["formulas_cached_only"]}
["附件3",null,"样衣参数"]
["序号","性别","每套配置","面料参数要求","工艺说明","单位","单人数量","总人数","样衣颜色要求","参考图片","投标报价 元/套（件）","投标面料参数","投标工艺说明","工艺要求\n（可高于或最新国家行业标准）"]
[1,"男 装","男装-西服上衣","可机洗抗变形羊毛：270g/m，成分：70%羊毛29.5聚酯纤维0.5%导电丝","男士外套：二扣，下双支线袋平袋盖，两端打“D”套结，后单开叉。领、手巾袋、袋盖门襟贡针0.15CM，袖口4扣，纽扣立体绕线。                               内：出头大挂面,内贡针,双支线袋两端D字套结,线同贡针颜色,里袋支线+三角+袋贴+汗托+袖里同大身里布.                          男士裤子：前门襟伸出宝剑头,内活动松紧腰,前无折,斜插袋,后单省,后双支线袋,六个裤袢,脚口锁边，有裤里,两侧口袋内缝加20cm加固线,后口袋三周压明线0.6cm,内门襟与活动口用裤袋布包边,内设专用防滑条，后浪内夹斜条外加锁边工艺，里腰下订针13个点。\n颜色要求：藏青色，见附件","件",1,146,"藏青色",{"$nulls":4},"男西装：执行GB 18401-2010、GB/T 2664-2017标准\n男裤：执行GB/T2666-2017标准\n女西装：执行GB 18401-2010、GB/T 2665-2017标准\n女裤：执行GB/T2666-2010标准\n男、女衬衫：执行GB 18401-2010、GB/T 2660-2017、GB/T 18863-2002标准"]
[2,null,"男装-配套西裤",null,null,"条",2,null,"藏青色"]
[3,null,"夏装西裤","凉感亲肤有微弹：  64%聚酯纤维30%冰凉玉6%氨纶","男士裤子：前门襟伸出宝剑头,内活动内松紧腰,前无折,斜插袋,后单省,后双支线袋,六个裤袢,脚口锁边                                      内：有裤里,两侧口袋内缝加20cm加固线,后口袋三周压明线0.6cm,内门襟与活动口用裤袋布包边,内设专用防滑条，后浪内夹斜条外加锁边工艺，里腰下订针13个点。","条",2,null,"藏青色"]
[4,null,"男装-长袖衬衫","100%棉液氨成衣免烫80S/2*80S/2,密度160*90","男士方领：压0.1cm止口明线,双层衬,领头插片.下领中3.0cm,单扣,单层衬、明门襟3cm宽,压0.1cm明线，里襟2.5cm宽,压明线、后担干压0.1cm明线，缝内放胶条衬，后背收双省不到底。袖窿圈压0.8cm明线，缝内放胶条衬，六角袖口6.5cm，斜角3cm，双排扣，止口压明线0.1cm，袖叉宽2.5cm，封头3.5cm，小袖叉1cm。单折,与袖克夫上口拼接缝上压0.1cm*0.8cm明线。前包后（埋夹工艺,缝内放胶条衬）。圆下摆卷边0.5cm，加胶条衬。","件",2,null,"白色"]
[5,null,"男装-短袖衬衫",null,null,"件",3,null,"白色"]
[6,"女 装","女装-西服上衣","可机洗抗变形羊毛：270g/m，成分：70%羊毛29.5聚酯纤维0.5%导电丝","女士外套：时尚修身版型，二扣,下两平双支线袋夹袋盖，前后片分割款式，圆下摆， 领子、门襟、袋盖贡针0.15CM，纽扣绕脚工艺。                                   内:出头直挂面,内贡针+支边,右边有暗口袋,洗唛车与暗口袋内,腋下收省,袋贴+里袋布+袖里同大身里布。                                                女士裤子：两侧松紧收腰4CM腰宽3CM,前门襟平腰头锁眼,前单省斜插袋,后单省无袋,六个裤袢,脚口锁边。                                内：有裤里,两侧口袋内缝加20cm加固线,后浪夹斜条外加锁边,内门襟用裤袋布包边,腰里两侧车织带                                ","件",1,null,"藏青色"]
[7,null,"女装-冬装西裤",null,null,"条",2,null,"藏青色"]
[8,null,"女装-夏装西裤","凉感亲肤有微弹：  64%聚酯纤维30%冰凉玉6%氨纶","女士裤子：两侧松紧收腰4CM腰宽3CM,前门襟平腰头锁眼,前单省斜插袋,后单省无袋,六个裤袢,脚口锁边。                                内：有裤里,两侧口袋内缝加20cm加固线,后浪夹斜条外加锁边,内门襟用裤袋布包边,腰里两侧车织带       ","条",2,null,"藏青色"]
[9,null,"女装-长袖衬衫","100%棉液氨成衣免烫80S/2*80S/2,密度160*90","女装方领,止口压0.1CM明线,下领中2.8CM,下领圆头单扣、双叠暗门襟2.5CM宽,压0.1CM明线,里襟2CM压明线,门襟活页打6个0.6cm套结，门襟条裁10cm宽、前片袖窿有腋下胸省，前+后片有收腰省至底摆、压0.5CM明线,缝内放胶条衬、袖窿圈压线0.7CM明线,缝内放胶条衬、直角5CM宽,订1粒扣,压0.1CM止口明线、\"V\"字型、单折与袖克夫上口拼接缝上压0.1cm*0.8cm明线、前包后(埋夹工艺,缝内放胶条衬)、圆下摆卷边0.5CM,加胶条衬","件",2,null,"白色"]
[10,null,"女装-短袖衬衫",null,null,"件",3,null,"白色"]
["投标总价"]
["备注：（总价包干），招标控制价420626元"]

{"sheet":"样衣模特数据参考","index":1,"n_rows":4,"n_cols":13,"rows_kept":4,"flags":["formulas_cached_only"]}
["样衣模特数据参考"]
["性别","身高","体重 ","净胸围","胸围","净中腰","中腰","净臀围","臀围","裤腰","裤长","肩宽","袖长"]
["女",165,98,82,null,68,null,87,null,67,98,43.5,56]
["男",177,69,null,90,null,81,null,104,null,105,49,64]